John's interaction with the events below:

	 14149  Pressed down
	 [ 17543] let up
	 [ 30325] Pressed down
	 35143 let up
	 39993 killed.
 
Compiled and uploaded: Wed Apr  1 15:07:20 PDT 2026

[ 12793][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x29
[ 12799][E][sd_diskio.cpp:806] sdcard_mount(): f_mount failed: (3) The physical drive cannot work
sample=3 state=BEGIN_FAIL rail=ON vbus=5.18 batt=0.00 pins=1/0/1/0 probeH(ff=8 z=0 o=0 FF FF FF FF) probeF(ff=8 z=0 o=0 FF FF FF FF) mount=none@0 type=NONE size=0MB root=FAIL
[ 13265][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x37
[ 13271][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x29
[ 13277][E][sd_diskio.cpp:806] sdcard_mount(): f_mount failed: (3) The physical drive cannot work
[ 13701][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x37
[ 13707][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x29
[ 13713][E][sd_diskio.cpp:806] sdcard_mount(): f_mount failed: (3) The physical drive cannot work
[ 14137][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x37
[ 14143][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x29
[ 14149][E][sd_diskio.cpp:806] sdcard_mount(): f_mount failed: (3) The physical drive cannot work
sample=4 state=MOUNT_OK rail=ON vbus=5.19 batt=0.00 pins=1/0/1/0 probeH(ff=8 z=0 o=0 FF FF FF FF) probeF(ff=8 z=0 o=0 FF FF FF FF) mount=HSPI@10000000 type=SDHC size=14910MB root=OK
sample=5 state=MOUNT_OK rail=ON vbus=5.18 batt=0.00 pins=1/0/1/0 probeH(ff=8 z=0 o=0 FF FF FF FF) probeF(ff=8 z=0 o=0 FF FF FF FF) mount=HSPI@400000 type=SDHC size=14910MB root=OK
sample=6 state=MOUNT_OK rail=ON vbus=5.18 batt=0.00 pins=1/0/1/0 probeH(ff=8 z=0 o=0 FF FF FF FF) probeF(ff=8 z=0 o=0 FF FF FF FF) mount=HSPI@400000 type=SDHC size=14910MB root=OK
sample=7 state=MOUNT_OK rail=ON vbus=5.18 batt=0.00 pins=1/0/1/0 probeH(ff=8 z=0 o=0 FF FF FF FF) probeF(ff=8 z=0 o=0 FF FF FF FF) mount=HSPI@400000 type=SDHC size=14910MB root=OK
sample=8 state=MOUNT_OK rail=ON vbus=5.18 batt=0.00 pins=1/0/1/0 probeH(ff=8 z=0 o=0 FF FF FF FF) probeF(ff=8 z=0 o=0 FF FF FF FF) mount=HSPI@400000 type=SDHC size=14910MB root=OK
sample=9 state=MOUNT_OK rail=ON vbus=5.18 batt=0.00 pins=1/0/1/0 probeH(ff=8 z=0 o=0 FF FF FF FF) probeF(ff=8 z=0 o=0 FF FF FF FF) mount=HSPI@400000 type=SDHC size=14910MB root=OK
sample=10 state=MOUNT_OK rail=ON vbus=5.18 batt=0.00 pins=1/0/1/0 probeH(ff=8 z=0 o=0 FF FF FF FF) probeF(ff=8 z=0 o=0 FF FF FF FF) mount=HSPI@400000 type=SDHC size=14910MB root=OK
sample=11 state=MOUNT_OK rail=ON vbus=5.18 batt=0.00 pins=1/0/1/0 probeH(ff=8 z=0 o=0 FF FF FF FF) probeF(ff=8 z=0 o=0 FF FF FF FF) mount=HSPI@400000 type=SDHC size=14910MB root=OK
sample=12 state=MOUNT_OK rail=ON vbus=5.18 batt=0.00 pins=1/0/1/0 probeH(ff=8 z=0 o=0 FF FF FF FF) probeF(ff=8 z=0 o=0 FF FF FF FF) mount=HSPI@400000 type=SDHC size=14910MB root=OK
sample=13 state=MOUNT_OK rail=ON vbus=5.18 batt=0.00 pins=1/0/1/0 probeH(ff=8 z=0 o=0 FF FF FF FF) probeF(ff=8 z=0 o=0 FF FF FF FF) mount=HSPI@400000 type=SDHC size=14910MB root=OK
sample=14 state=MOUNT_OK rail=ON vbus=5.18 batt=0.00 pins=1/0/1/0 probeH(ff=8 z=0 o=0 FF FF FF FF) probeF(ff=8 z=0 o=0 FF FF FF FF) mount=HSPI@400000 type=SDHC size=14910MB root=OK
sample=15 state=MOUNT_OK rail=ON vbus=5.18 batt=0.00 pins=1/0/1/0 probeH(ff=8 z=0 o=0 FF FF FF FF) probeF(ff=8 z=0 o=0 FF FF FF FF) mount=HSPI@400000 type=SDHC size=14910MB root=OK
sample=16 state=MOUNT_OK rail=ON vbus=5.18 batt=0.00 pins=1/0/1/0 probeH(ff=8 z=0 o=0 FF FF FF FF) probeF(ff=8 z=0 o=0 FF FF FF FF) mount=HSPI@400000 type=SDHC size=14910MB root=OK
[ 17543][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0xsample=17 state=MOUNT_OK rail=ON vbus=5.18 batt=0.00 pins=1/0/1/0 probeH(ff=8 z=0 o=0 FF FF FF FF) probeF(ff=8 z=0 o=0 FF FF FF FF) mount=HSPI@400000 type=SDHC size=14910MB root=OK
37
[ 17549][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x29
[ 17555][E][sd_diskio.cpp:806] sdcard_mount(): f_mount failed: (3) The physical drive cannot work
[ 17979][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x37
[ 17985][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x29
[ 17991][E][sd_diskio.cpp:806] sdcard_mount(): f_mount failed: (3) The physical drive cannot work
[ 18415][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x37
[ 18421][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x29
[ 18427][E][sd_diskio.cpp:806] sdcard_mount(): f_mount failed: (3) The physical drive cannot work
[ 18851][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x37
[ 18857][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x29
[ 18863][E][sd_diskio.cpp:806] sdcard_mount(): f_mount failed: (3) The physical drive cannot work
[ 19287][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x37
[ 19293][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x29
[ 19299][E][sd_diskio.cpp:806] sdcard_mount(): f_mount failed: (3) The physical drive cannot work
[ 19723][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x37
[ 19729][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x29
[ 19735][E][sd_diskio.cpp:806] sdcard_mount(): f_mount failed: (3) The physical drive cannot work
[ 20159][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x37
[ 20165][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x29
[ 20171][E][sd_diskio.cpp:806] sdcard_mount(): f_mount failed: (3) The physical drive cannot work
[ 20595][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x37
[ 20601][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x29
[ 20607][E][sd_diskio.cpp:806] sdcard_mount(): f_mount failed: (3) The physical drive cannot work
sample=18 state=BEGIN_FAIL rail=ON vbus=5.18 batt=0.00 pins=1/0/1/0 probeH(ff=8 z=0 o=0 FF FF FF FF) probeF(ff=8 z=0 o=0 FF FF FF FF) mount=none@0 type=NONE size=0MB root=FAIL
[ 21073][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x37
[ 21079][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x29
[ 21085][E][sd_diskio.cpp:806] sdcard_mount(): f_mount failed: (3) The physical drive cannot work
[ 21509][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x37
[ 21515][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x29
[ 21521][E][sd_diskio.cpp:806] sdcard_mount(): f_mount failed: (3) The physical drive cannot work
[ 21945][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x37
[ 21951][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x29
[ 21957][E][sd_diskio.cpp:806] sdcard_mount(): f_mount failed: (3) The physical drive cannot work
[ 22381][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x37
[ 22387][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x29
[ 22393][E][sd_diskio.cpp:806] sdcard_mount(): f_mount failed: (3) The physical drive cannot work
[ 22817][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x37
[ 22823][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x29
[ 22829][E][sd_diskio.cpp:806] sdcard_mount(): f_mount failed: (3) The physical drive cannot work
[ 23253][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x37
[ 23259][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x29
[ 23265][E][sd_diskio.cpp:806] sdcard_mount(): f_mount failed: (3) The physical drive cannot work
[ 23689][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x37
[ 23695][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x29
[ 23701][E][sd_diskio.cpp:806] sdcard_mount(): f_mount failed: (3) The physical drive cannot work
[ 24125][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x37
[ 24131][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x29
[ 24137][E][sd_diskio.cpp:806] sdcard_mount(): f_mount failed: (3) The physical drive cannot work
[ 24603][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0xsample=19 state=BEGIN_FAIL rail=ON vbus=5.19 batt=0.00 pins=1/0/1/0 probeH(ff=8 z=0 o=0 FF FF FF FF) probeF(ff=8 z=0 o=0 FF FF FF FF) mount=none@0 type=NONE size=0MB root=FAIL
37
[ 24609][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x29
[ 24615][E][sd_diskio.cpp:806] sdcard_mount(): f_mount failed: (3) The physical drive cannot work
[ 25039][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x37
[ 25045][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x29
[ 25051][E][sd_diskio.cpp:806] sdcard_mount(): f_mount failed: (3) The physical drive cannot work
[ 25475][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x37
[ 25481][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x29
[ 25487][E][sd_diskio.cpp:806] sdcard_mount(): f_mount failed: (3) The physical drive cannot work
[ 25911][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x37
[ 25917][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x29
[ 25923][E][sd_diskio.cpp:806] sdcard_mount(): f_mount failed: (3) The physical drive cannot work
[ 26347][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x37
[ 26353][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x29
[ 26359][E][sd_diskio.cpp:806] sdcard_mount(): f_mount failed: (3) The physical drive cannot work
[ 26783][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x37
[ 26789][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x29
[ 26795][E][sd_diskio.cpp:806] sdcard_mount(): f_mount failed: (3) The physical drive cannot work
[ 27219][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x37
[ 27225][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x29
[ 27231][E][sd_diskio.cpp:806] sdcard_mount(): f_mount failed: (3) The physical drive cannot work
[ 27655][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x37
[ 27661][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x29
[ 27667][E][sd_diskio.cpp:806] sdcard_mount(): f_mount failed: (3) The physical drive cannot work
sample=20 state=BEGIN_FAIL rail=ON vbus=5.19 batt=0.00 pins=1/0/1/0 probeH(ff=8 z=0 o=0 FF FF FF FF) probeF(ff=8 z=0 o=0 FF FF FF FF) mount=none@0 type=NONE size=0MB root=FAIL
[ 28133][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x37
[ 28139][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x29
[ 28145][E][sd_diskio.cpp:806] sdcard_mount(): f_mount failed: (3) The physical drive cannot work
[ 28569][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x37
[ 28575][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x29
[ 28581][E][sd_diskio.cpp:806] sdcard_mount(): f_mount failed: (3) The physical drive cannot work
[ 29005][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x37
[ 29011][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x29
[ 29017][E][sd_diskio.cpp:806] sdcard_mount(): f_mount failed: (3) The physical drive cannot work
[ 29441][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x37
[ 29447][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x29
[ 29453][E][sd_diskio.cpp:806] sdcard_mount(): f_mount failed: (3) The physical drive cannot work
[ 29877][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x37
[ 29883][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x29
[ 29889][E][sd_diskio.cpp:806] sdcard_mount(): f_mount failed: (3) The physical drive cannot work
[ 30313][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x37
[ 30319][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x29
[ 30325][E][sd_diskio.cpp:806] sdcard_mount(): f_mount failed: (3) The physical drive cannot work
sample=21 state=MOUNT_OK rail=ON vbus=5.19 batt=0.00 pins=1/0/1/0 probeH(ff=8 z=0 o=0 FF FF FF FF) probeF(ff=8 z=0 o=0 FF FF FF FF) mount=FSPI@4000000 type=SDHC size=14910MB root=OK
sample=22 state=MOUNT_OK rail=ON vbus=5.18 batt=0.00 pins=1/0/1/0 probeH(ff=8 z=0 o=0 FF FF FF FF) probeF(ff=8 z=0 o=0 FF FF FF FF) mount=HSPI@400000 type=SDHC size=14910MB root=OK
sample=23 state=MOUNT_OK rail=ON vbus=5.18 batt=0.00 pins=1/0/1/0 probeH(ff=8 z=0 o=0 FF FF FF FF) probeF(ff=8 z=0 o=0 FF FF FF FF) mount=HSPI@400000 type=SDHC size=14910MB root=OK
sample=24 state=MOUNT_OK rail=ON vbus=5.18 batt=0.00 pins=1/0/1/0 probeH(ff=8 z=0 o=0 FF FF FF FF) probeF(ff=8 z=0 o=0 FF FF FF FF) mount=HSPI@400000 type=SDHC size=14910MB root=OK
sample=25 state=MOUNT_OK rail=ON vbus=5.18 batt=0.00 pins=1/0/1/0 probeH(ff=8 z=0 o=0 FF FF FF FF) probeF(ff=8 z=0 o=0 FF FF FF FF) mount=HSPI@400000 type=SDHC size=14910MB root=OK
sample=26 state=MOUNT_OK rail=ON vbus=5.18 batt=0.00 pins=1/0/1/0 probeH(ff=8 z=0 o=0 FF FF FF FF) probeF(ff=8 z=0 o=0 FF FF FF FF) mount=HSPI@400000 type=SDHC size=14910MB root=OK
sample=27 state=MOUNT_OK rail=ON vbus=5.18 batt=0.00 pins=1/0/1/0 probeH(ff=8 z=0 o=0 FF FF FF FF) probeF(ff=8 z=0 o=0 FF FF FF FF) mount=HSPI@400000 type=SDHC size=14910MB root=OK
sample=28 state=MOUNT_OK rail=ON vbus=5.18 batt=0.00 pins=1/0/1/0 probeH(ff=8 z=0 o=0 FF FF FF FF) probeF(ff=8 z=0 o=0 FF FF FF FF) mount=HSPI@400000 type=SDHC size=14910MB root=OK
sample=29 state=MOUNT_OK rail=ON vbus=5.18 batt=0.00 pins=1/0/1/0 probeH(ff=8 z=0 o=0 FF FF FF FF) probeF(ff=8 z=0 o=0 FF FF FF FF) mount=HSPI@400000 type=SDHC size=14910MB root=OK
sample=30 state=MOUNT_OK rail=ON vbus=5.18 batt=0.00 pins=1/0/1/0 probeH(ff=8 z=0 o=0 FF FF FF FF) probeF(ff=8 z=0 o=0 FF FF FF FF) mount=HSPI@400000 type=SDHC size=14910MB root=OK
sample=31 state=MOUNT_OK rail=ON vbus=5.18 batt=0.00 pins=1/0/1/0 probeH(ff=8 z=0 o=0 FF FF FF FF) probeF(ff=8 z=0 o=0 FF FF FF FF) mount=HSPI@400000 type=SDHC size=14910MB root=OK
sample=32 state=MOUNT_OK rail=ON vbus=5.18 batt=0.00 pins=1/0/1/0 probeH(ff=8 z=0 o=0 FF FF FF FF) probeF(ff=8 z=0 o=0 FF FF FF FF) mount=HSPI@400000 type=SDHC size=14910MB root=OK
sample=33 state=MOUNT_OK rail=ON vbus=5.18 batt=0.00 pins=1/0/1/0 probeH(ff=8 z=0 o=0 FF FF FF FF) probeF(ff=8 z=0 o=0 FF FF FF FF) mount=HSPI@400000 type=SDHC size=14910MB root=OK
sample=34 state=MOUNT_OK rail=ON vbus=5.18 batt=0.00 pins=1/0/1/0 probeH(ff=8 z=0 o=0 FF FF FF FF) probeF(ff=8 z=0 o=0 FF FF FF FF) mount=HSPI@400000 type=SDHC size=14910MB root=OK
sample=35 state=MOUNT_OK rail=ON vbus=5.18 batt=0.00 pins=1/0/1/0 probeH(ff=8 z=0 o=0 FF FF FF FF) probeF(ff=8 z=0 o=0 FF FF FF FF) mount=HSPI@400000 type=SDHC size=14910MB root=OK
sample=36 state=MOUNT_OK rail=ON vbus=5.18 batt=0.00 pins=1/0/1/0 probeH(ff=8 z=0 o=0 FF FF FF FF) probeF(ff=8 z=0 o=0 FF FF FF FF) mount=HSPI@400000 type=SDHC size=14910MB root=OK
sample=37 state=MOUNT_OK rail=ON vbus=5.18 batt=0.00 pins=1/0/1/0 probeH(ff=8 z=0 o=0 FF FF FF FF) probeF(ff=8 z=0 o=0 FF FF FF FF) mount=HSPI@400000 type=SDHC size=14910MB root=OK
sample=38 state=MOUNT_OK rail=ON vbus=5.18 batt=0.00 pins=1/0/1/0 probeH(ff=8 z=0 o=0 FF FF FF FF) probeF(ff=8 z=0 o=0 FF FF FF FF) mount=HSPI@400000 type=SDHC size=14910MB root=OK
sample=39 state=MOUNT_OK rail=ON vbus=5.18 batt=0.00 pins=1/0/1/0 probeH(ff=8 z=0 o=0 FF FF FF FF) probeF(ff=8 z=0 o=0 FF FF FF FF) mount=HSPI@400000 type=SDHC size=14910MB root=OK
sample=40 state=MOUNT_OK rail=ON vbus=5.18 batt=0.00 pins=1/0/1/0 probeH(ff=8 z=0 o=0 FF FF FF FF) probeF(ff=8 z=0 o=0 FF FF FF FF) mount=HSPI@400000 type=SDHC size=14910MB root=OK
[ 35143][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0xsample=41 state=MOUNT_OK rail=ON vbus=5.18 batt=0.00 pins=1/0/1/0 probeH(ff=8 z=0 o=0 FF FF FF FF) probeF(ff=8 z=0 o=0 FF FF FF FF) mount=HSPI@400000 type=SDHC size=14910MB root=OK
37
[ 35149][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x29
[ 35155][E][sd_diskio.cpp:806] sdcard_mount(): f_mount failed: (3) The physical drive cannot work
[ 35579][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x37
[ 35585][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x29
[ 35591][E][sd_diskio.cpp:806] sdcard_mount(): f_mount failed: (3) The physical drive cannot work
[ 36015][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x37
[ 36021][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x29
[ 36027][E][sd_diskio.cpp:806] sdcard_mount(): f_mount failed: (3) The physical drive cannot work
[ 36451][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x37
[ 36457][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x29
[ 36463][E][sd_diskio.cpp:806] sdcard_mount(): f_mount failed: (3) The physical drive cannot work
[ 36887][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x37
[ 36893][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x29
[ 36899][E][sd_diskio.cpp:806] sdcard_mount(): f_mount failed: (3) The physical drive cannot work
[ 37323][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x37
[ 37329][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x29
[ 37335][E][sd_diskio.cpp:806] sdcard_mount(): f_mount failed: (3) The physical drive cannot work
[ 37759][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x37
[ 37765][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x29
[ 37771][E][sd_diskio.cpp:806] sdcard_mount(): f_mount failed: (3) The physical drive cannot work
[ 38195][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x37
[ 38201][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x29
[ 38207][E][sd_diskio.cpp:806] sdcard_mount(): f_mount failed: (3) The physical drive cannot work
sample=42 state=BEGIN_FAIL rail=ON vbus=5.18 batt=0.00 pins=1/0/1/0 probeH(ff=8 z=0 o=0 FF FF FF FF) probeF(ff=8 z=0 o=0 FF FF FF FF) mount=none@0 type=NONE size=0MB root=FAIL
[ 38673][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x37
[ 38679][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x29
[ 38685][E][sd_diskio.cpp:806] sdcard_mount(): f_mount failed: (3) The physical drive cannot work
[ 39109][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x37
[ 39115][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x29
[ 39121][E][sd_diskio.cpp:806] sdcard_mount(): f_mount failed: (3) The physical drive cannot work
[ 39545][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x37
[ 39551][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x29
[ 39557][E][sd_diskio.cpp:806] sdcard_mount(): f_mount failed: (3) The physical drive cannot work
[ 39981][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x37
[ 39987][E][sd_diskio.cpp:199] sdCommand(): Card Failed! cmd: 0x29
[ 39993][E][sd_diskio.cpp:806] sdcard_mount(): f_mount failed: (3) The physical drive cannot work
(rnsenv) jlpoole@jp /usr/local/src/microreticulum/microReticulumTbeam $ date
Wed Apr  1 15:08:35 PDT 2026
(rnsenv) jlpoole@jp /usr/local/src/microreticulum/microReticulumTbeam $ 